The OSM designdata contain:

1. schematic
	- Cadence library (fs_osm.olb) including:
		- general OSM symbol (V1.1, V1.2, size S)
		- symbols of F&S OSM modules (module-specific implementation information)
		- F&S OSM spacer symbol
		- F&S OSM heatspreader symbol (p.n. & scope of supply)

	- Altium library (fs_osm.SchLib) including:
		- general OSM Size S symbol (V1.2)
		- symbols of F&S OSM modules (module-specific implementation information)
		- F&S OSM spacer symbol

2. pcb
	- Cadence
		- fs_osm_lga332_1p25_30x30_bb.dra:
			footprint of OSM module (baseboard side, include position references for the spacers, suitable for the use of the F&S OSM heatspreader Rev.1.10)
		- fs_osm_spacer_m2p5_3p0.dra
			footprint of OSM spacer

	- Altium library (OSM_Size_S_V120.PcbLib) including
		- general OSM Size S symbol (V1.2)
		- F&S OSM spacer symbol

3. 3D
	- 3D model of FS 8ULP OSM-SF_REV100
	- 3D model of FS 8ULP OSM-SF_REV110
	- 3D model of FS IMX93 OSM-SF_REV100
	- 3D model of FS IMX93 OSM-SF_REV110
	- 3D model of FS 8MM OSM-SF_REV110
	- 3D model of FS 8MM OSM-SF_REV120
	- 3D model of FS 8MP OSM-SF_REV100
	- 3D model of FS 8MP OSM-SF_REV110
	- 3D model of Heatspreader MHS.OSM.1 